IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "IFC.ifc"
Time stamp: "2015-11-27T17:12:57"
Author: "Patrick"
Organization: "None"
Preprocessor: "15.0.0"
Originating system: "ETABS 2015"
Authorization: "None"
Application: "ETABS 2015" version "15.0.0" identifier "ETABS 2015" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER)

People and organizations
  Person "Nameless" id "Patrick" of Organization "None" (roles: STRUCTURALENGINEER)
  Owner history of Person "Nameless" id "Patrick" of Organization "None" (roles: STRUCTURALENGINEER) | application "ETABS 2015" version "15.0.0" identifier "ETABS 2015" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER) | change NOCHANGE | created 1448644377 (2015-11-27T17:12:57Z) | last modified 1448644377 (2015-11-27T17:12:57Z)
  Owner history of Person "Nameless" id "Patrick" of Organization "None" (roles: STRUCTURALENGINEER) | application "ETABS 2015" version "15.0.0" identifier "ETABS 2015" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER) | change MODIFIED | created 1448644377 (2015-11-27T17:12:57Z) | last modified 1448644377 (2015-11-27T17:12:57Z)

Units
  LENGTHUNIT: INCH (conversion based)
  AREAUNIT: SQUARE INCH (conversion based)
  VOLUMEUNIT: CUBIC INCH (conversion based)
  SECTIONMODULUSUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: SLINCH (conversion based)
  MASSDENSITYUNIT: derived
  FORCEUNIT: LBF (conversion based)
  TORQUEUNIT: derived
  PRESSUREUNIT: PSI (conversion based)
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  LINEARMOMENTUNIT: derived
  SHEARMODULUSUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  THERMODYNAMICTEMPERATUREUNIT: FAHRENHEIT (conversion based)
  THERMALEXPANSIONCOEFFICIENTUNIT: derived

Spatial structure
IFCPROJECT "ETABS_File.$et"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "BASE LEVEL" | elevation 0.0000000E+000
        contains 16 elements
          16 x IFCCOLUMN | names: "1", "2", "3" (+13 more) | material: "A992Fy50"
      IFCBUILDINGSTOREY "LEVEL 2" | elevation 1.9200000E+002
        contains 40 elements
          16 x IFCCOLUMN | names: "17", "18", "19" (+13 more) | material: "A992Fy50"
          24 x IFCBEAM | names: "97", "98", "99" (+21 more) | material: "A992Fy50"
      IFCBUILDINGSTOREY "LEVEL 3" | elevation 3.6000000E+002
        contains 40 elements
          16 x IFCCOLUMN | names: "33", "34", "35" (+13 more) | material: "A992Fy50"
          24 x IFCBEAM | names: "73", "74", "75" (+21 more) | material: "A992Fy50"
      IFCBUILDINGSTOREY "TOP LEVEL" | elevation 5.2800000E+002
        contains 24 elements
          24 x IFCBEAM | names: "49", "50", "51" (+21 more) | material: "A992Fy50"